On Calibrating a Projector-Camera Rig to Enable Spatial Augmented Reality Use Cases Using cpsspatialar

Michael Hornacek

TU Vienna (IMW-CPS)

May 2021

# Motivation

Spatial augmented reality (SAR) is a branch of augmented reality whereby the augmentation of the scene is carried out using a projector. While pointing a projector at a scene and projecting an image is on its own not a challenge, doing so in a manner such that the projected content **appear to be** **naturally part of the scene** is more tricky. The intuition for the general problem we face can be drawn from using a projector to project an image to a flat wall: unless the projector faces the wall frontally, the bounds of a projected rectangular image will not appear rectangular, but more generally as a trapezoid (i.e., the image will appear distorted). The cause for this effect is that the geometry of the scene as it relates to the geometry of the projector plays a role in *how the pixels of the projector’s image plane map to points in the scene*.

The central **objective** we set for ourselves is to **enable correcting for distortion** caused by projecting to arbitrary scene geometry in an **automatic** fashion. This is to be done in a manner that lends itself to practical application in a real-world setting where the **scene** to be augmented—e.g., an **object** being gradually assembled and its **placement** relative to the projector—**does not remain static**. Moreover, the object in question may but may not in its entirety fall within the projector’s **field of view (FOV)**. Finally, the solution is ideally to rely on the existing **hardware setup**—i.e., projector with steerable mirror system and stereo camera—mounted in the Pilotfabrik[[1]](#footnote-1) of TU Vienna.

# Approach

The problem of correcting for distortions as outlined in Section 1 requires knowledge of the manner in which the respective rays through the pixels of the projector’s image plane fan out into the scene, and the geometry of the scene itself within at least the projector’s field of view (determined in part by the steerable mirror),[[2]](#footnote-2) as illustrated in Figure 1. This is because the scene point ‘illuminated’ by a pixel in the projector’s image plane is given by intersecting its corresponding ray with the geometry of the scene surface. To model this interaction calls for two components in particular: (i) one-time **projector calibration** and (ii) **recovery of** **scene geometry** whenever the scene undergoes change relative to the field of view of the projector.




Figure 1: Projector-scene geometry. The way rays ‘fan out’ through the pixels of the projector’s image plane is given by calibrating the projector (note that the projector’s field of view is the portion of the scene in between the gray rays). The scene point ‘illuminated’ by a pixel in the projector’s image plane is given by intersecting its corresponding ray with the geometry of the scene surface. Projector calibration and recovery of scene geometry are accordingly prerequisites of the image warping that it is our ambition to carry out.

The remainder of this section is organized in accordance with these two components: one-time projector calibration, and recovery of scene geometry.

## One-time Projector Calibration

The ‘output’ of projector calibration[[3]](#footnote-3) is a mathematical model that determines, for each pixel **x**proj in the projector’s image plane *π*proj, the ray from the projector’s center of projection **C**proj through **x**proj, along which the pixel is projected *to the scene*. Inversely, the model also determines the projection **x**’proj of any point **X**’proj in the scene *to the projector’s image plane* *π*proj, obtained by intersecting *π*proj with the ray from **C**proj through **X**’proj. Such a model is said to function in accordance with the principle of **central projection**.




Figure 2: Pinhole camera model. The image plane π is perpendicular to the Z axis of the camera’s coordinate frame; its location is given by the focal length f, the distance of π along the Z axis. The camera’s center of projection **C** is located at the origin **0** of the camera coordinate frame. The projection **x** = (xcam, ycam) of a point **X** = (X, Y, Z) to π, by central projection, follows from the principle of similar triangles. Note that the origin of the coordinate system of the image plane—called the principal point—is situated at the intersection of the Z axis with π. Note that the Z component of a point expressed in the camera’s coordinate frame is referred to as the point’s depth relative to the camera.

Notably, central projection is the same principle that underlies the modelling of conventional cameras. A camera modeled in accordance with the principle of central projection is called a **pinhole camera**. A pinhole camera—as illustrated in Figure 2—can be expressed in terms of a 3 × 3 ‘camera calibration’ matrix **K**,[[4]](#footnote-4) derived from the camera’s focal length and principal point. In practice, a pinhole camera model works well in modelling how the respective rays through the pixels of the image plane fan out into the scene, on the condition that images to which the model is applied have been corrected for **lens** **distortions** caused by the camera’s lens system (cf. Figure 3 for an example). The ‘output’ of camera calibration is accordingly typically not only the matrix **K**, but the associated **lens distortions model coefficients** as well. The lens distortion model coefficients enable applying a lens distortion model to **undistort** any image acquired by the camera.

In practice, calibrating a *camera* relies on (i) establishing **2D-3D correspondences** between pixels in the camera’s image plane and corresponding points in the scene, and on (ii) using those correspondences as input to an **optimization procedure** that outputs the calibration matrix **K** and the associated distortion model coefficients. Calibration of a *projector* can be carried out in precisely the same manner insofar as step (ii) is concerned; *the major difference in projector calibration relative to camera calibration concerns the manner in which 2D-3D correspondences are identified*, i.e.,between pixels in the image plane of the projector and the corresponding points in the scene.

What remains of this section first reviews how 2D-3D correspondences are conventionally obtained between camera and scene. Next, we address how we proceed to obtain 2D-3D correspondences between projector and scene. Finally, we outline the manner in which 2D-3D correspondences are used to compute the calibration matrix **K** and associated lens distortion model coefficients. Camera and projector calibration are **implemented in cpsspatialar as described** in this section, respectively, by the apps calibrateCam (which is capable of calibrating a single camera or a stereo pair) and calibrateProj (which takes a camera calibration produced by calibrateCam as input).

### Obtaining Camera-Scene 2D-3D Correspondences

The recovery of 2D-3D correspondences in support of camera calibration is carried out, conventionally, by relying on a planar **calibration surface** of known **scale** to automatically identify correspondences between the 3D points on the calibration surface and their 2D correspondences in the image plane. A widely used example of such a calibration object is a **chessboard pattern**.[[5]](#footnote-5) The 3D **corner points** of the chessboard are obtained analytically in a coordinate system defined in the plane of the chessboard, requiring knowledge only of the length of a side of a chessboard square.[[6]](#footnote-6) Next, using the findChessboardCorners() function in OpenCV[[7]](#footnote-7) the corresponding 2D pixels of the corner points in any single image of the chessboard are obtained as a list; an example is given in Figure 3.

In practice, multiple images of the chessboard are acquired, from a set of **widely varying viewpoints**.[[8]](#footnote-8) The rationale behind doing so is to capture the varying effects of lens distortion across the full extent of the camera’s field of view; notably, images of the chessboard acquired only at approximately the middle of the image plane would fail to provide information about radial distortions present at the image plane’s boundaries.




Figure 3: 2D chessboard corners recovered automatically using OpenCV’s findChessboardCorners() function, color coded using the drawChessboardCorners() function. The corresponding 3D positions can be computed analytically, given prior knowledge of the length of a square of the chessboard. Note the distortions caused by the camera’s lens system, clearly visible in the image: the edges of the chessboard should be straight lines, but instead appear to bend outwards.

### Obtaining Projector-Scene 2D-3D Correspondences

We obtain 3D points via intersection with ground plane of back-projections of detected circles projected to the floor, with the corresponding 2D points known a priori in the coordinate system of the circles pattern we feed to the projector. Besides recovering the intrinsics of the projector, for each of the locations on the floor to which we project and thereby for precisely the respective projector look directions, we will obtain the extrinsics of the projector. These will be the projector look directions for which we will be able to carry out spatial AR.

|  |  |
| --- | --- |
| (a) | (b) |

Figure 4: todo... (a) Projected circle pattern, with 2D circle centers obtained using again the function findChessboardCorners(), color coded using drawChessboardCorners(). (b) The corresponding 3D locations on the ground of the circle centers for any image of the circle pattern are obtained by computing the intersection of the ground plane (recovered by camera resection with respect to the known **K** of the camera—obtained by calibrating the camera in a prior step—and 2D-3D correspondences with respect to the chessboard pattern placed on the floor) with the back-projections of the detected circle centers …

### Computing the Calibration

Given a set of 2D-3D correspondences in the form of a list of lists[[9]](#footnote-9) of 2D pixel positions (‘image points’) and a corresponding list of 3D points (‘object points’), the OpenCV[[10]](#footnote-10) function calibrateCamera() can be used to carry out the actual calibration. The function returns the camera calibration matrix **K** and the lens distortion model coefficients.[[11]](#footnote-11) Additionally, the function returns a list of 3D rigid body transformations whose length equals the number of calibration images used as input; the *n*th such rigid body transformation gives the pose (**R**, **t**) of the camera or projector relative to the corresponding 3D points as seen in the *n*th calibration image.[[12]](#footnote-12) The projection of such a 3D point **X** to the image plane of the camera or projector with respect to the *n*th calibration image is given by **K**(**RX** + **t**), and is obtained in a manner such that, collectively over all 2D-3D correspondences, the sum of squared distances[[13]](#footnote-13) in the image plane between the 2D projections of these 3D points and their respective 2D correspondence are minimized.

## Computing the Warp

*Todo: the discussion of stereo here is relevant to the case where we want to project to arbitrary surface geometry. We will pursue this as out next step (and then texture map the resulting mesh). For our first step (projecting to a flat surface), we get the ground plane using a checkerboard pattern…*

### Planar Scene Geometry

*Todo… Warp via* ***plane-induced homography*** *with respect to ground plane, viewpoint of virtual projector, and viewpoint of original projector…*

### Arbitrary Scene Geometry

Fundamental to all variants of stereo is that, given a pixel **x** in the left image, the search for the corresponding pixel **x**’ in the right image is restricted to only pixels situated along the **epipolar line** spanned by **x**, as illustrated in Figure 5. *Where stereo approaches differ is primarily in how the ‘best’ match along an epipolar line is determined.* Classical **correlation-based** stereo approaches rely on maximizing a similarity score over a window about **x** in the left image and the corresponding windows about respective candidate matching pixel in the right image. However, a correlation-based approach can be expected to work well only in the presence of adequately **discriminative texture**.[[14]](#footnote-14) A way around this is to *introduce* discriminative texture by projecting a pattern to the scene.

*Warp via* ***texture mapping*** *recovered mesh from viewpoint of virtual projector, and rendering resulting textured mesh from viewpoint of original projector…*





Figure 5: Epipolar geometry (i.e., the geometry of stereo). The 3D point **X** that projects to the pixel **x** in the left camera’s image plane must lie along the ray passing through **x** from the left camera’s center of projection **C**. Accordingly, the projection **x**’ of **X** to the image plane of the right camera must lie along the epipolar line **l**’ spanned by **x**, obtained by projecting that ray to the right camera’s image plane. This restricts the search for **x**’ to only the pixels along that line, a constraint common to all stereo approaches. Once **x**’ has been identified, the point **X** can be recovered by triangulation.


# Building the Code

Let CPSSPATIALAR\_BASEDIR refer to the base directory of your local copy the **cpsspatialar** Git repository[[15]](#footnote-15) (such that src and docs are subdirectories of CPSSPATIALAR\_BASEDIR):

1. Install **Visual Studio Professional 2019**[[16]](#footnote-16)
2. Install **CMake**[[17]](#footnote-17)
3. Install **Git**[[18]](#footnote-18)
4. Let VCPKG\_BASEDIR refer to HOME\_DIR/vcpkg; install **vcpkg**[[19]](#footnote-19), having cloned from within HOME\_DIR (such that vcpkg.exe is then located in VCPKG\_BASEDIR)
5. Set[[20]](#footnote-20) the environment variable CMAKE\_TOOLCHAIN\_FILE to point to VCPKG\_BASEDIR\scripts\buildsystems\vcpkg.cmake
6. Add VCPKG\_BASEDIR to the system’s PATH environment variable
7. Let EIGEN\_BASEDIR refer to CPSSPATIALAR\_BASEDIR\src\external\eigen;[[21]](#footnote-21) download version 3.4 of the source code of **Eigen**[[22]](#footnote-22) and extract to EIGEN\_BASEDIR (such that the CMakeLists.txt file is located in EIGEN\_BASEDIR)
8. Let OPENCV\_BASEDIR refer to CPSSPATIALAR\_BASEDIR\src\external\opencv; download version 4.5.1 of the source code of **OpenCV**[[23]](#footnote-23) and extract to OPENCV\_BASEDIR (such that the CMakeLists.txt file is located in OPENCV\_BASEDIR)
9. Run CMake (cmake-gui):



1. Enter OPENCV\_BASEDIR in the field to the right of ‘Where is the source code’ and OPENCV\_BASEDIR\build in the field to the right of ‘Where to build the binaries’ (note that backslashes are converted automatically to forward slashes)
2. Click ‘Configure’ and click ‘Yes’ if prompted to create the directory OPENCV\_BASEDIR
3. If prompted to specify the generator for this project and to optionally indicate the platform for the generator, provide ‘Visual Studio 16 2019’ and ‘x64’, respectively, and click ‘Finish’
4. Click ‘Open Project’ or, equivalently, open OPENCV\_BASEDIR\build\OpenCV.sln; this opens the Visual Studio solution OpenCV.sln in Visual Studio Professional 2019
5. Select ‘Release’ from the Solution Configuration pull-down menu and select ‘Build:Build Solution’ from the menu bar to finally build (i.e., compile) OpenCV in release mode (note that it will take some minutes for building to complete):



1. Add CPSSPATIALAR\_BASEDIR\src\external\opencv\build\bin\Release to the system’s PATH environment variable

1. Let FREEGLUT\_BASEDIR refer to CPSSPATIALAR\_BASEDIR\src\external\ freeglut; download version 2.8.1 of **freeglut**[[24]](#footnote-24) pre-built binaries to FREEGLUT\_BASEDIR (such that the CMakeLists.txt file is located in FREEGLUT\_BASEDIR)
2. Let GLEW\_BASEDIR refer to CPSSPATIALAR\_BASEDIR\src\external\glew; download version 2.1.0 of the source code of **glew**[[25]](#footnote-25) and extract to GLEW\_BASEDIR (such that the Makefile file is located in GLEW\_BASEDIR)
3. Run CMake (cmake-gui)
4. Enter GLEW\_BASEDIR\build\cmake in the field to the right of ‘Where is the source code’ and GLEW\_BASEDIR in the field to the right of ‘Where to build the binaries’ (note that backslashes are converted automatically to forward slashes)
5. Click ‘Configure’
6. If prompted to specify the generator for this project and to optionally indicate the platform for the generator, provide ‘Visual Studio 16 2019’ and ‘x64’, respectively, and click ‘Finish’
7. Click ‘Open Project’ or, equivalently, open GLEW\_BASEDIR\glew.sln; this opens the Visual Studio solution glew.sln in Visual Studio Professional 2019
8. Select ‘Release’ from the Solution Configuration pull-down menu and select ‘Build:Build Solution’ from the menu bar to build glew in release mode
9. Let GLFW\_BASEDIR refer to CPSSPATIALAR\_BASEDIR\src\external\glfw; download version 3.3.4 of the source code of **glfw**[[26]](#footnote-26) and extract to GLFW\_BASEDIR (such that the Makefile file is located in GLFW\_BASEDIR)
10. Run CMake (cmake-gui)
11. Enter GLFW\_BASEDIR in the field to the right of ‘Where is the source code’ and GLFW\_BASEDIR\build in the field to the right of ‘Where to build the binaries’ (note that backslashes are converted automatically to forward slashes)
12. Click ‘Configure’
13. If prompted to specify the generator for this project and to optionally indicate the platform for the generator, provide ‘Visual Studio 16 2019’ and ‘x64’, respectively, and click ‘Finish’
14. Click ‘Open Project’ or, equivalently, open GLFW\_BASEDIR\glfw.sln; this opens the Visual Studio solution glew.sln in Visual Studio Professional 2019
15. Select ‘Release’ from the Solution Configuration pull-down menu and select ‘Build:Build Solution’ from the menu bar to build glfw in release mode
16. Open the terminal and run vcpkg install --triplet=x64-windows pcl followed by vcpkg integrate install to install **PCL** (Point Cloud Library)[[27]](#footnote-27) to make it discoverable by Visual Studio, respectively
17. Open the terminal and run vcpkg install --triplet=x64-windows ceres followed by vcpkg integrate install to install **Google Ceres**[[28]](#footnote-28) to make it discoverable by Visual Studio, respectively
18. Run CMake (cmake-gui)
19. Enter CPSSPATIALAR\_BASEDIR\src in the field to the right of ‘Where is the source code’ and CPSSPATIALAR\_BASEDIR\build in the field to the right of ‘Where to build the binaries’ (note that backslashes are converted automatically to forward slashes)
20. Click ‘Configure’ and click ‘Yes’ if prompted to create the directory CPSSPATIALAR\_BASEDIR
21. If prompted to specify the generator for this project and to optionally indicate the platform for the generator, provide ‘Visual Studio 16 2019’ and ‘x64’, respectively, select ‘Specify toolchain file for cross-compiling’, and click ‘Next’
22. Enter VCPKG\_BASEDIR\scripts\buildsystems\vcpkg.cmake as the path to the toolchain file and click ‘Finish’
23. Click ‘Open Project’ or, equivalently, open CPSSPATIALAR\_BASEDIR\build\cpspatialar.sln; this opens the Visual Studio solution cpspatialar.sln in Visual Studio Professional 2019
24. Select ‘Release’ from the Solution Configuration pull-down menu and select ‘Build:Build Solution’ from the menu bar to build cpsspatialar in release mode

The **resulting executables** can be found at CPSSPATIALAR\_BASEDIR\build\bin\Release

# Running the Code

See the repository for sample data sets. Invocations are provided in associated .bat files.

## Notes on Camera Calibration

When acquiring images for camera calibration, it is essential to capture images of the pattern **across the image plane** (sides, middle), yet making sure the pattern always remain **fully visible** in the acquired images. For best results, also acquire images of the pattern at **varying depths** relative to the camera; at the very least, make sure to acquire images with the pattern placed on the floorplane (or whatever the target surface is), since we want the system to be well calibrated for at least the target surface.

## Notes on Projector Calibration

1. <https://www.pilotfabrik.at/?lang=en> [↑](#footnote-ref-1)
2. Cf. Section 4.1.2 of the Spatial Augmented Reality textbook of Bimber and Raskar, available at <http://pages.cs.wisc.edu/~dyer/cs534/papers/SAR.pdf>. Note that the authors also mention **user location**; this is relevant for some—but not all—use cases, and we shall leave it too outside the scope of this document. [↑](#footnote-ref-2)
3. Cf. again Section 4.1.2 of Bimber and Raskar. [↑](#footnote-ref-3)
4. If you’ll forgive a brazen bit of self-indulgence, have a look at Chapter 2 of my dissertation at <https://publik.tuwien.ac.at/files/PubDat_243668.pdf> for a more detailed attempt at a self-contained but accessible introduction to the geometry pinhole cameras, the derivation of the camera calibration matrix **K**, and other topics of relevance to this document (including epipolar geometry). [↑](#footnote-ref-4)
5. Cf. <https://markhedleyjones.com/projects/calibration-checkerboard-collection> for a variety of chessboard calibration patterns ready for use. [↑](#footnote-ref-5)
6. E.g., (0,0,0), (1.5,0,0), (3,0,0), …, (9,7.5,0) for a chessboard with 7 × 6 corners, with each square of length and width of 1.5 unit, respectively. [↑](#footnote-ref-6)
7. See <https://docs.opencv.org/master/dc/dbb/tutorial_py_calibration.html> for a comprehensive tutorial. [↑](#footnote-ref-7)
8. It is good practice to acquire images of the calibration surface across all corners and edges of the image plane, along with an image or two from around the middle of the image plane. Beware: for any given viewpoint, the *entirety* of the chessboard must be visible if relying on OpenCV’s findChessboardCorners(). Otherwise, the function will fail to find any corners in the image acquired from that viewpoint. [↑](#footnote-ref-8)
9. Each list contains a list corresponding to each respective image. [↑](#footnote-ref-9)
10. See again <https://docs.opencv.org/master/dc/dbb/tutorial_py_calibration.html> for a comprehensive tutorial. [↑](#footnote-ref-10)
11. See <https://www.learnopencv.com/understanding-lens-distortion/> for more details on how these particular coefficients are interpreted mathematically. [↑](#footnote-ref-11)
12. Note that if these points are of a calibration surface placed on the floor, then such a rigid body transformation gives the pose of the projector or camera relative to the ‘**ground plane**’; the inverse of this rigid body transformation gives the pose of the ground plane relative to the projector or camera. [↑](#footnote-ref-12)
13. Such residuals are referred to as **reprojection errors** in computer vision. [↑](#footnote-ref-13)
14. Objects like the white walls of a room *or typical manmade objects* are too poorly textured to enable reliable matching via correlation-based stereo. [↑](#footnote-ref-14)
15. <https://github.com/m-hornacek/cpsspatialar> [↑](#footnote-ref-15)
16. Available via TU Wien Campus Software at <https://www.it.tuwien.ac.at/en/services/software/software-provision/campus-software/>. [↑](#footnote-ref-16)
17. Via Windows win64-x64 Installer at <https://cmake.org/download/> [↑](#footnote-ref-17)
18. Via Windows 64 bit installer at <https://git-scm.com/download/win> (use all standard options) [↑](#footnote-ref-18)
19. <https://vcpkg.io/en/getting-started.html> [↑](#footnote-ref-19)
20. In other words, “assign” or “create”… [↑](#footnote-ref-20)
21. Note that here as for all subdirectories of CPSSPATIALAR\_BASEDIR\src\external, it is critical that the naming of the subdirectories is exactly as indicated in these instructions. [↑](#footnote-ref-21)
22. <https://gitlab.com/libeigen/eigen/-/archive/3.4/eigen-3.4.zip> [↑](#footnote-ref-22)
23. <https://github.com/opencv/opencv/archive/4.5.1.zip> [↑](#footnote-ref-23)
24. <https://www.transmissionzero.co.uk/files/software/development/GLUT/older/freeglut-MSVC-2.8.1-1.mp.zip> [↑](#footnote-ref-24)
25. <https://sourceforge.net/projects/glew/files/glew/2.1.0/glew-2.1.0.zip/download> [↑](#footnote-ref-25)
26. <https://github.com/glfw/glfw/releases/download/3.3.4/glfw-3.3.4.zip> [↑](#footnote-ref-26)
27. <https://pointclouds.org/> [↑](#footnote-ref-27)
28. <http://ceres-solver.org/> [↑](#footnote-ref-28)